**Ground Hog HD Specifications and Features**

**SPECIFICATIONS**

|  |  |
| --- | --- |
| Auger Speed | 140 rpm @ 3600 engine rpm (no load) |
| Auger Torque | **275 ft. lbs. torque** (approximate) |
| Maximum Depth | **Depends on length of Auger** |
| Weight | **295 lbs.** (134 kg) (with fluids) |
| Length | **Normal Drilling 100 inches**(253 cm) |
| Length | **Close-up Drilling 75 inches** (190 cm) |
| Width | **34 inches** (86 cm) |
| Height | **38 inches** (96 cm) |
| Shipping | **80L X 48W X 47H Weight 412 lbs**  |
| Drill Bit Size | **7/8" square** |

**FEATURES**

* 9hp Honda engine
* Digs holes up to 18 inches in diameter
* Hydraulics variable auger speed and reverse
* Almost perfectly balanced with an 8-inch auger
* Right angle design to eliminate torque to the operator
* 3 handlebar positions
* Pivoting drilling head for drilling on uneven terrain
* Large highway rated tires
* Locking mechanism on the digging head for easy storage during jobsite maneuvering
* Heavy duty powder coated steel construction
* Pivoting engine cradle that helps keep the engine level and protects the engine with proper oiling angle
* Low profile and compact design of the frame allows the unit to be transported in the bed of a small truck.
* Towbar with a 2" hitch coupler and safety chains for surface street and jobsite transport.